**СПЕЦИФІКАЦІЯ SIEMENS**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **№п/п** |  | **Назва** | **Заказний номер** | **Кількість, шт** |
| 1 |  | Запобіжники 400А | 3NE3 332-0B | 6 |
| 2 |  | Центральний процесор CPU 315 | 6ES7315-2EH14-0AB0 | 2 |
| 3 |  | карта памяті |  6ES7953-8LJ31-0AA0 | 2 |
| 4 |  | Центральний процесор CPU 317 | 6ES7317-2AK14-0AB0 | 1 |
| 5 |  | Центральний процесор CPU 317 | 6ES7317-2EK14-0AB0 | 1 |
| 6 |  | Карта пам’яті 2MB RAM | 6ES7953-8LL31-0AA0 | 2 |
| 7 |  | OP панель | 6AV2 124-0JC01-0AX0 | 2 |
| 8 |  | Плавний пуск | 3RW5546-6HA14 | 1 |
| 9 |  | DP/DP repeater | 6es7972-0AB01-0XA0 | 3 |
| 10 |  | БЛОК ЖИВЛЕННЯ SIMATIC S7-300 | 6ES7307-1EA01-0AA0 | 5 |
| 11 |  | модуль DIx32 |  6ES7321-1BL00-0AA0 | 3 |
| 12 |  | кабель сигнальний мідний з роз'ємом з одного боку 40х0,5  | 6ES7922-3ВD20-0AC0 | 5 |
| 13 |  | ІНТЕРФЕЙСНИЙ МОДУЛЬ ДЛЯ КОНТРОЛЕРА ET200M |  6ES7153-1AA03-0XB0  | 3 |
| 14 |  | Модуль АО8 | 6ES7 332-5HF00-0AB0 | 3 |
| 15 |  | Перетворювач температури | 7NG3212-0NN00 | 15 |
| 16 |  | Електропневматичний позиціонер | 6DR5010-0NG00-0AA0 | 5 |
| 17 |  | OP панель | 6AV2 124-1GC01-0AX0 | 1 |
| 18 |  | Комунікаційний процесор | 6GK7 343-1CX10-0XE0 | 2 |
| 19 |  | **Перетворювач тиску**SITRANS P320 Pressure transmitter Gauge pressure HART (4...20 mA) Measuring cell filling: Silicone oil Maximum measuring span: 250 mbar (3.6 psi) Male thread G1/2 (DIN EN 837-1) Process connection: Stainless steel 316L/1.4404, Seal diaphragms: Stainless steel 316L/1.4404, Sensor differential pressure: Process flange: Stainless steel 316/1.4408 Die-cast aluminum housing Dual chamber device no Ex 2 x M20 x 1.5 With display (lid with glass window) Cable gland and sealing plug attached, metal General approval without Ex approval: World (CE, UKCA, RCM) except: CSA, EAC, FM, KC Mounting bracket, stainless steel 1.4301/304 Process connection male thread G1/2, opening 11 mm Measuring range setting: Lower range value (max. 5 characters), Upper range value (max. 5 characters), Unit (mbar, bar, kPa, MPa, psi, ...) Example: -0.5 ... 10.5 psi (stainless steel plate) {Y01: -100 ... 100 mbar} | 7MF0300-1FD01-5AF2-Z A01+E00+H02+K80+Y01 | 12 |
| 20 |  | ГАЗОАНАЛІЗАТОР | 7MB2338-0AD16-3NL1-Z A13 | 1 |
| 21 |  | Панель оператора | 6AV6646-1BA22-1AA1 | 1 |
|  |  |  |  |  |
|  |  |  |  |  |